Ref:3622/TOK/G.22/ June 27, 2022

**CORRIGENDUM**

**Ref. Tender No. TRA-Tocklai/22-23/T-02 Dated 17.06.2022**

With reference to the Tender Notification as mentioned hereinabove published in the news papers and uploaded in the official website [www.tocklai.org](http://www.tocklai.org), the following Corrigendum is hereby made in Annexure-A:

**Annexure – A**

**SPECIFICATIONS OF EQUIPMENTS/ INSTRUMENTS**

|  |  |  |  |
| --- | --- | --- | --- |
| **Sl. No.** | **Items** | **Unit No.** | **Revised Specifications** |
| 1. | **Lyophilizer** | 01 | **Standard make:**  Ice Holding Capacity: 2liters, Cold Trap  Temperature: -86° C  Drying chamber size: Ø160 x 230mm,  Cylindrical made of thick gauge 304 Grade Stainless Steel, 4 port for drying with 4 quick seal  valves.  Cold trap size:160mm x 100mm, cylindrical, made of thick gauge 304 grade stainless steel,  External Vacuum Pump: 2 stage direct drive  Vacuum Indication: Pirani gauge  Vacuum Level: 0.5 to 0.002 mbar  Microprocessor based controller with Digital Display, PT 100 sensor  Temperature resolution: 1° C  Controls: Refrigeration ON/OFF, Vacuum ON/OFF  Exterior: Powder coated mild steel.  Built In CFC free refrigeration system  Cascade Refrigeration System  Facility for water drain  2nos of 250ml conical flask, cork, and glass adaptors included with  the supply  Power supply: 230 V, 50 Hz, single phase |
| 2. | **Digital Lab Balance** | 01 | **Standard make:**  High Precision Lab, Scale (3 digit after decimal)  Vibration resistant |
| 3. | **pH Meter** | 01 | **Standard make:**  3 Point calibration, Stability : 0.002 pH per hour  Accuracy : + 1mV + 1 Digit,  Temperature Compensation : Auto/Mnual mV Range : 0 to +1999.9 mV  Accessories :  (i) pH Electrode (Combined)  (ii) Temperature Probe (PT 100 Sensor)  (iii) Electrode Stand & Clamp/ Beaker. |
| 4. | **Digital Outdoor Weighing Balance** | 01 | **Standard make:**  Capacity 10 Kg |

**Last date of issue/receipt of tenders is extended to: 21.07.2022 up to 5.00 p.m.**

**All other Terms & Conditions of Tender No. TRA-Tocklai/22-23/T-02 Dated 17.06.2022 will remain the same.**

**DIRECTOR**